New Function in Firmware V1.0.01-250121(SFU)

This Firmware has SFU mode as default!!

These settings need to be made in the XGSPON OLT-2XG(S)

1. Now you can use the OLT to set the ONU Firewall to control the Attack Protection:
(1) OLT set ONU Firewall Disable: ONU Firewall low and disable the attack protection.
(2) OLT set ONU Firewall Low: ONU Firewall low and enable the attack protection.
(3) OLT set ONU Firewall High: ONU Firewall high and enable the attack portection
See image 1 for location in OLT.

2. Now you can use the OLT to change the ONU work at SFU/HGU mode (Change mode will make ONU reboot).
   Do not use Auto in the menu with the ONU-10XGS-1004-10G, only select either HGU or SFU.
See image 2 for location in OLT.


After the Firmware Update has been completed, 
Reset the ONU to Factory Default settings for the best results.
When the ONU has already been added to the OLT, its best to either refesh or
delete the ONU from the OLT and re-register it. 
