Building Image
================================================================================
OS:
	Fedora 8 (Fedora-8-i386-DVD.iso) - test ok


Prepare:
	1. Install Fedora 8 and select all of software development tools

Building:
	1. Build process require 'root' privileges
	2. cd /home
	3. tar jvx mt7620-AirliveGpl-20151225.tar.gz
	4. cd /home/mt7620-AirliveGpl
	5. make menuconfig;
		If see the configuration screen, directly exit and save
		Image path: ./image/BR6477OAC/UPG/BR6477OAC_Airlive_x.xx_upg.bin

Covered under Ralink protection:
	1. hw_nat.ko
	2. rlt_wifi.ko
	3. rt2860v2_ap.ko

non-GPL
	1. easyedx
	2. edx_*
	3. lighttpd*